# SR61T

Interleaved 2 of 5 - Enable  
  
<SW>444001

Interleaved 2 of 5 - Barcode length - Length mode - L1 as min, L2 as max  
  
<SW>445302

Interleaved 2 of 5 - Barcode length - Set lengths 1, 2 and 3 - Compose L1: 4  
  
<SW>445004

Interleaved 2 of 5 - Barcode length - Set lengths 1, 2 and 3 - Compose L2: 20  
  
<SW>445114